## AS6500 Assembler

####

    ACKNOWLEDGMENT

       Thanks  to  Marko  Makela  for his contribution of the AS6500
    cross assembler.

            Marko Makela
            Sillitie 10 A
            01480 Vantaa
            Finland
            Internet: Marko.Makela@Helsinki.Fi
            EARN/BitNet: msmakela@finuh

       Several  additions and modifications were made to his code to
    support the following families of 6500 processors:

            (1)     650X and 651X processor family
            (2)     65F11 and 65F12 processor family
            (3)     65C00/21 and 65C29 processor family
            (4)     65C02, 65C102, and 65C112 processor family

       The  instruction  syntax of this cross assembler contains two
    peculiarities:  (1) the addressing indirection is denoted by the
    square  brackets  []  and (2) the `bbrx' and `bbsx' instructions
    are written `bbr0 memory,label'.

####

    6500 REGISTER SET

    The following is a list of the 6500 registers used by AS6500:

            a       -       8-bit accumulator
            x,y     -       index registers

    6500 INSTRUCTION SET

       The  following  tables  list all 6500 family mnemonics recog-
    nized by the AS6500 assembler.  The designation [] refers  to  a
    required addressing mode argument.  The following list specifies
    the format for each addressing mode supported by AS6500:

            #data           immediate data
                            byte or word data

            *dir            direct page addressing
                            (see .setdp directive)
                            0 <= dir <= 255

            offset,x        indexed addressing
            offset,y        indexed addressing
                            address = (offset + (x or y))

            [offset,x]      pre-indexed indirect addressing
                            0 <= offset <= 255
                            address = contents of location
                                (offset + (x or y)) mod 256

            [offset],y      post-indexed indirect addressing
                            address = contents of location at offset
                                plus the value of the y register

            [address]       indirect addressing

            ext             extended addressing

            label           branch label

            address,label   direct page memory location
                            branch label
                            bbrx and bbsx instruction addressing

    The  terms data, dir, offset, address, ext, and label may all be
    expressions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the 65xx technical data for valid modes.

    Processor Specific Directives

       The  AS6500  cross  assembler has four (4) processor specific
    assembler directives which  define  the  target  65xx  processor
    family:

            .r6500          Core 650X and 651X family (default)
            .r65f11         Core plus 65F11 and 65F12
            .r65c00         Core plus 65C00/21 and 65C29
            .r65c02         Core plus 65C02, 65C102, and 65C112

    65xx Core Inherent Instructions

            brk                     clc
            cld                     cli
            clv                     dex
            dey                     inx
            iny                     nop
            pha                     php
            pla                     plp
            rti                     rts
            sec                     sed
            sei                     tax
            tay                     tsx
            txa                     txs
            tya

    65xx Core Branch Instructions

            bcc     label           bhs     label
            bcs     label           blo     label
            beq     label           bmi     label
            bne     label           bpl     label
            bvc     label           bvs     label

    65xx Core Single Operand Instructions

            asl     []
            dec     []
            inc     []
            lsr     []
            rol     []
            ror     []

    65xx Core Double Operand Instructions

            adc     []
            and     []
            bit     []
            cmp     []
            eor     []
            lda     []
            ora     []
            sbc     []
            sta     []

    65xx Core Jump and Jump to Subroutine Instructions

            jmp     []              jsr     []

    65xx Core Miscellaneous X and Y Register Instructions

            cpx     []
            cpy     []
            ldx     []
            stx     []
            ldy     []
            sty     []

    65F11 and 65F12 Specific Instructions

            bbr0    [],label                bbr1    [],label
            bbr2    [],label                bbr3    [],label
            bbr4    [],label                bbr5    [],label
            bbr6    [],label                bbr7    [],label

            bbs0    [],label                bbs1    [],label
            bbs2    [],label                bbs3    [],label
            bbs4    [],label                bbs5    [],label
            bbs6    [],label                bbs7    [],label

            rmb0    []                      rmb1    []
            rmb2    []                      rmb3    []
            rmb4    []                      rmb5    []
            rmb6    []                      rmb7    []

            smb0    []                      smb1    []
            smb2    []                      smb3    []
            smb4    []                      smb5    []
            smb6    []                      smb7    []

    65C00/21 and 65C29 Specific Instructions

            bbr0    [],label                bbr1    [],label
            bbr2    [],label                bbr3    [],label
            bbr4    [],label                bbr5    [],label
            bbr6    [],label                bbr7    [],label

            bbs0    [],label                bbs1    [],label
            bbs2    [],label                bbs3    [],label
            bbs4    [],label                bbs5    [],label
            bbs6    [],label                bbs7    [],label

            bra     label

            phx                             phy
            plx                             ply

            rmb0    []                      rmb1    []
            rmb2    []                      rmb3    []
            rmb4    []                      rmb5    []
            rmb6    []                      rmb7    []

            smb0    []                      smb1    []
            smb2    []                      smb3    []
            smb4    []                      smb5    []
            smb6    []                      smb7    []

    65C02, 65C102, and 65C112 Specific Instructions

            bbr0    [],label                bbr1    [],label
            bbr2    [],label                bbr3    [],label
            bbr4    [],label                bbr5    [],label
            bbr6    [],label                bbr7    [],label

            bbs0    [],label                bbs1    [],label
            bbs2    [],label                bbs3    [],label
            bbs4    [],label                bbs5    [],label
            bbs6    [],label                bbs7    [],label

            bra     label

            phx                             phy
            plx                             ply

            rmb0    []                      rmb1    []
            rmb2    []                      rmb3    []
            rmb4    []                      rmb5    []
            rmb6    []                      rmb7    []

            smb0    []                      smb1    []
            smb2    []                      smb3    []
            smb4    []                      smb5    []
            smb6    []                      smb7    []

            stz     []
            trb     []
            tsb     []

       Additional  addressing  modes for the following core instruc-
    tions are also available with the 65C02, 65C102, and 65C112 pro-
    cessors.

            adc     []                      and     []
            cmp     []                      eor     []
            lda     []                      ora     []
            sbc     []                      sta     []

            bit     []                      jmp     []

            dec                             inc

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: April 2009