## ASST7 Assembler

####

    ST7 REGISTER SET

    The following is a list of the ST7 registers used by ASST7:

            a       -       8-bit accumulator
            x,y     -       8-bit index registers
            cc      -       8-bit condition code register
            s       -       16-bit stack pointer

    ST7 INSTRUCTION SET

         The following list specifies the format for each addressing
    mode supported by ASST7:

            reg             register addressing
                            (a,x,y,s,cc)

            #data           immediate data byte

            *saddr          8-bit zero page addressing
                            0x00 <= dir <= 0xFF

            laddr           16-bit addressing

            (x)             register indirect addressing

            (*sofst,r)      short indexed (r = x,y)
            (sofst,r).b

            (lofst,r).w     long indexed (r = x,y)

            (ofst,r)        if ofst is relocatable or
                            an external value then
                            the (lofst,r).w mode is
                            selected by default
                            else

            (ofst,r)        if ofst is a locally
                            defined constant then
                            the (sofst,r).b mode
                            is selected when
                            0x00 <= ofst <= 0xFF else
                            the (lofst,r).w mode
                            is selected

                            Instructions supporting
                            only a single form will
                            use the appropriate form
                            but will report an error.

            [*saddr]        short indirect
            [saddr].b

            [laddr].w       long indexed

            [addr]          if addr is relocatable or
                            an external value then
                            the [laddr].w mode is
                            selected by default
                            else

            [addr]          if addr is a locally
                            defined constant then
                            the [saddr].b mode
                            is selected when
                            0x00 <= addr <= 0xFF else
                            the [laddr].w mode
                            is selected

                            Instructions supporting
                            only a single form will
                            use the appropriate form
                            but will report an error.

            ([*saddr],r)    short indirect indexed
            ([saddr].b,r)   (r = x,y)
            ([saddr],r).b

            ([laddr].w,r)   long indirect indexed
            ([laddr],r).w   (r = x,y)

            ([addr],r)      if addr is relocatable or
                            an external value then
                            the ([laddr],r).w mode is
                            selected by default
                            else

            ([addr],r)      if addr is a locally
                            defined constant then
                            the ([saddr],r).b mode
                            is selected when
                            0x00 <= addr <= 0xFF else
                            the ([laddr],r).w mode
                            is selected

                            Instructions supporting
                            only a single form will
                            use the appropriate form
                            but will report an error.

            label           pc-relative branch addressing

    The  terms  data,  saddr,  laddr,  addr, sofst, lofst, ofst, and
    label may all be expressions.

         Note that not all addressing modes are valid with every in-
    struction, refer to the ST7 technical data for valid modes.
    The  following  tables  list all ST7 mnemonics recognized by the
    ASST7 assembler.  The designation [] refers to  a  required  ad-
    dressing mode argument.

    Inherent Instructions

            nop                     trap
            wfi                     halt
            ret                     iret
            sim                     rim
            scf                     rcf
            rsp

    Conditional Branch Instructions

            jra     label
            jrt     label           jrf     label
            jrih    label           jril    label
            jrh     label           jrnh    label
            jrm     label           jrnm    label
            jrmi    label           jrpl    label
            jreq    label           jrne    label
            jrc     label           jrnc    label
            jrult   label           jruge   label
            jrugt   label           jrule   label

            jra     [saddr]
            jrt     [saddr]         jrf     [saddr]
            jrih    [saddr]         jril    [saddr]
            jrh     [saddr]         jrnh    [saddr]
            jrm     [saddr]         jrnm    [saddr]
            jrmi    [saddr]         jrpl    [saddr]
            jreq    [saddr]         jrne    [saddr]
            jrc     [saddr]         jrnc    [saddr]
            jrult   [saddr]         jruge   [saddr]
            jrugt   [saddr]         jrule   [saddr]

    Bit Test and Branch Instructions

            btjt    saddr,#,label
            btjf    saddr,#,label
            btjt    [saddr],#,label
            btjf    [saddr],#,label

    Bit Manipulation Instructions

            bset    saddr,#
            bres    saddr,#
            bset    [saddr],#
            bres    [saddr],#

    Single Operand Instructions

            neg     []              cpl     []
            srl     []              rrc     []
            sra     []              rlc     []
            sll     []              sla     []
            dec     []              inc     []
            tnz     []              swap    []
            clr     []

            pop     reg             push    reg

    Double Operand Instructions

            add     a,[]            adc     a,[]
            and     a,[]            bcp     a,[]
            or      a,[]            sbc     a,[]
            sub     a,[]            xor     a,[]

            mul     x,a             mul     y,a

            cp      reg,[]

            ld      [],[]

    Call to Subroutine and Jump Instructions

            call    []              jp      []

            callr   label           callr   [saddr]

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: October 2010