## ASF2MC8 Assembler

####

    PROCESSOR SPECIFIC DIRECTIVES

       The ASF2MC8 assembler supports the F2MC8L and F2MC8FX proces-
    sor cores.

    .8L Directive

    Format:

            .8L

    The  .8L  directive selects the F2MC8L processor cycle counts to
    be listed when the -c option is specified.  This is the  default
    selection  if  no processor directive is specified in the source
    assemby file.

    .8FX Directive

    Format:

            .8FX

    The .8FX directive selects the F2MC8FX processor cycle counts to
    be listed when the -c option is specified.  .8L is  the  default
    selection  if  no processor directive is specified in the source
    assemby file.

    The .__.CPU.  Variable

       The value of the pre-defined symbol '.__.CPU.' corresponds to
    the selected processor type.  The default value is 0 which  cor-
    responds  to  the  default  processor type.  The following table
    lists the processor types and associated values for the  ASF2MC8
    assembler:

            Processor Type            .__.CPU. Value
            --------------            --------------
                .8L                          0
                .8FX                         1

       The  variable  '.__.CPU.'  is by default defined as local and
    will not be output to the created .rel file.  The assembler com-
    mand line options -g or -a will not cause the local symbol to be
    output to the created .rel file.

       The  assembler  .globl  directive  may  be used to change the
    variable type to global causing its definition to be  output  to
    the  .rel file.  The inclusion of the definition of the variable
    '.__.CPU.' might be a useful means of validating that seperately
    assembled  files have been compiled for the same processor type.
    The linker will report an error for variables with multiple  non
    equal definitions.

    F2MC8L/F2MC8FX REGISTERS

       The  following  is a list of register designations recognized
    by the ASF2MC8 assembler:

            pc              -       Program Counter

            a               -       Accumulator

            t               -       Temporary Accumulator

            ix              -       Index Register

            ep              -       Extra Pointer

            sp              -       Stack Pointer

            ps              -       Program Status

            r0,r1,r2,r3,    -       Memory Registers
            r4,r5,r6,r7             32 banks of
                                    8 registers each

    F2MC8L/F2MC8FX INSTRUCTION SET

       The  following  list specifies the format for each addressing
    mode supported by ASF2MC8:

            #data           immediate data
                            byte or word data

            *dir            direct page addressing

            *dir:b          bit addressing to a
                            direct page address

            ext             extended addressing

            a,t             register addressing
            pc,sp,ix,ep

            @a              accumulator indexed

            @ix+d           indexed addressing
                            plus offset

            @ix             indexed addressing
                            with a zero offset

            @ep             pointer addressing

            r               General-purpose registers

            label           call/jmp/branch label

    The  terms  data,  dir,  ext, b, d, and label may all be expres-
    sions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the F2MC8L/F2MC8FX technical data for  valid
    modes.

       The following tables list all F2MC8L/F2MC8FX mnemonics recog-
    nized by the ASF2MC8 assembler.  The designation [] refers to  a
    required addressing mode argument.

    Transfer Instructions

            mov     [],[]           movw    [],[]
            xch     [],[]           xchw    [],[]
            clrb    []              setb    []
            swap    []

    Operation Instructions

            addc    a(,[])          addcw   a
            subc    a(,[])          subcw   a
            inc     r               incw    []
            dec     r               decw    []
            mulu    a               divu    a
            and     a(,[])          andw    a
            cmp     a(,[])          cmpw    a
            or      a(,[])          orw     a
            xor     a(,[])          xorw    a
            rolc    a               rorc    a
            daa                     das

    Branch/Jump/Call Instructions

            bz      label           bew     label
            bnz     label           bne     label
            bc      label           blo     label
            bnc     label           bhs     label
            bn      label           bp      label
            blt     label           bge     label
            bbc     *dir:b,label    bbs     *dir:b,label
            jmp     []              call    label
            callv   #data           xchw    a,pc
            ret                     reti

    Other Instructions

            pushw   []              popw    []
            nop
            clrc                    setc
            clri                    seti

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: April 2009