## AS6809 Assembler

####

    6809 REGISTER SET

    The following is a list of the 6809 registers used by AS6809:

            a,b     -       8-bit accumulators
            d       -       16-bit accumulator <a:b>
            x,y     -       index registers
            s,u     -       stack pointers
            pc      -       program counter
            cc      -       condition code
            dp      -       direct page

    6809 INSTRUCTION SET

       The  following  tables  list all 6809 mnemonics recognized by
    the AS6809 assembler.  The designation [] refers to  a  required
    addressing  mode  argument.   The  following  list specifies the
    format for each addressing mode supported by AS6809:

            #data           immediate data
                            byte or word data

            *dir            direct page addressing
                            (see .setdp directive)
                            0 <= dir <= 255

            label           branch label

            r,r1,r2         registers
                            cc,a,b,d,dp,x,y,s,u,pc

            ,-x     ,--x    register indexed
                            autodecrement

            ,x+     ,x++    register indexed
                            autoincrement

            ,x              register indexed addressing
                            zero offset

            offset,x        register indexed addressing
                               -16 <= offset <= 15    ---  5-bit
                              -128 <= offset <= -17   ---  8-bit
                                16 <= offset <= 127   ---  8-bit
                            -32768 <= offset <= -129  --- 16-bit
                               128 <= offset <= 32767 --- 16-bit
                            (external definition of offset
                             uses 16-bit mode)

            a,x             accumulator offset indexed addressing

            ext             extended addressing

            ext,pc          pc addressing ( pc <- pc + ext )

            ext,pcr         pc relative addressing

            [,--x]          register indexed indirect
                            autodecrement

            [,x++]          register indexed indirect
                            autoincrement

            [,x]            register indexed indirect addressing
                            zero offset

            [offset,x]      register indexed indirect addressing
                              -128 <= offset <= 127   ---  8-bit
                            -32768 <= offset <= -129  --- 16-bit
                               128 <= offset <= 32767 --- 16-bit
                            (external definition of offset
                             uses 16-bit mode)

            [a,x]           accumulator offset indexed
                            indirect addressing

            [ext]           extended indirect addressing

            [ext,pc]        pc indirect addressing
                            ( [pc <- pc + ext] )

            [ext,pcr]       pc relative indirect addressing

    The  terms  data, dir, label, offset, and ext may all be expres-
    sions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the 6809 technical data for valid modes.

    Inherent Instructions

            abx             daa
            mul             nop
            rti             rts
            sex             swi
            swi1            swi2
            swi3            sync

    Short Branch Instructions

            bcc     label           bcs     label
            beq     label           bge     label
            bgt     label           bhi     label
            bhis    label           bhs     label
            ble     label           blo     label
            blos    label           bls     label
            blt     label           bmi     label
            bne     label           bpl     label
            bra     label           brn     label
            bvc     label           bvs     label
            bsr     label

    Long Branch Instructions

            lbcc    label           lbcs    label
            lbeq    label           lbge    label
            lbgt    label           lbhi    label
            lbhis   label           lbhs    label
            lble    label           lblo    label
            lblos   label           lbls    label
            lblt    label           lbmi    label
            lbne    label           lbpl    label
            lbra    label           lbrn    label
            lbvc    label           lbvs    label
            lbsr    label

    Single Operand Instructions

            asla            aslb
            asl     []

            asra            asrb
            asr     []

            clra            clrb
            clr     []

            coma            comb
            com     []

            deca            decb
            dec     []

            inca            incb
            inc     []

            lsla            lslb
            lsl     []

            lsra            lsrb
            lsr     []

            nega            negb
            neg     []

            rola            rolb
            rol     []

            rora            rorb
            ror     []

            tsta            tstb
            tst     []

    Double Operand Instructions

            adca    []              adcb    []

            adda    []              addb    []

            anda    []              andb    []

            bita    []              bitb    []

            cmpa    []              cmpb    []

            eora    []              eorb    []

            lda     []              ldb     []

            ora     []              orb     []

            sbca    []              sbcb    []

            sta     []              stb     []

            suba    []              subb    []

    D-register Instructions

            addd    []              subd    []
            cmpd    []              ldd     []
            std     []

    Index/Stack Register Instructions

            cmps    []              cmpu    []
            cmpx    []              cmpy    []

            lds     []              ldu     []
            ldx     []              ldy     []

            leas    []              leau    []
            leax    []              leay    []

            sts     []              stu     []
            stx     []              sty     []

            pshs    r               pshu    r
            puls    r               pulu    r

    Jump and Jump to Subroutine Instructions

            jmp     []              jsr     []

    Register - Register Instructions

            exg     r1,r2           tfr     r1,r2

    Condition Code Register Instructions

            andcc   #data           orcc    #data
            cwai    #data

    6800 Compatibility Instructions

            aba             cba
            clc             cli
            clv             des
            dex             ins
            inx
            ldaa    []      ldab    []
            oraa    []      orab    []
            psha            pshb
            pula            pulb
            sba             sec
            sei             sev
            staa    []      stab    []
            tab             tap
            tba             tpa
            tsx             txs
            wai

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: April 2009