## AS6811 Assembler

####

    68HC11 REGISTER SET

    The following is a list of the 68HC11 registers used by AS6811:

            a,b     -       8-bit accumulators
            d       -       16-bit accumulator <a:b>
            x,y     -       index registers

    68HC11 INSTRUCTION SET

       The  following tables list all 68HC11 mnemonics recognized by
    the AS6811 assembler.  The designation [] refers to  a  required
    addressing  mode  argument.   The  following  list specifies the
    format for each addressing mode supported by AS6811:

            #data           immediate data
                            byte or word data

            *dir            direct page addressing
                            (see .setdp directive)
                            0 <= dir <= 255

            ,x              register indirect addressing
                            zero offset

            offset,x        register indirect addressing
                            0 <= offset <= 255

            ext             extended addressing

            label           branch label

    The terms data, dir, offset, and ext may all be expressions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the 68HC11 technical data for valid modes.

    Inherent Instructions

            aba             abx
            aby             cba
            clc             cli
            clv             daa
            des             dex
            dey             fdiv
            idiv            ins
            inx             iny
            mul             nop
            rti             rts
            sba             sec
            sei             sev
            stop            swi
            tab             tap
            tba             tpa
            tsx             txs
            wai             xgdx
            xgdy

            psha            pshb
            psh a           psh b
            pshx            pshy
            psh x           psh y

            pula            pulb
            pul a           pul b
            pulx            puly
            pul x           pul y

    Branch Instructions

            bra     label           brn     label
            bhi     label           bls     label
            bcc     label           bhs     label
            bcs     label           blo     label
            bne     label           beq     label
            bvc     label           bvs     label
            bpl     label           bmi     label
            bge     label           blt     label
            bgt     label           ble     label
            bsr     label

    Single Operand Instructions

            asla            aslb            asld
            asl a           asl b           asl d
            asl     []

            asra            asrb
            asr a           asr b
            asr     []

            clra            clrb
            clr a           clr b
            clr     label

            coma            comb
            com a           com b
            com     []

            deca            decb
            dec a           dec b
            dec     []

            inca            incb
            inc a           inc b
            inc     []

            lsla            lslb            lsld
            lsl a           lsl b           lsl d
            lsl     []

            lsra            lsrb            lsrd
            lsr a           lsr b           lsr d
            lsr     []

            nega            negb
            neg a           neg b
            neg     []

            rola            rolb
            rol a           rol b
            rol     []

            rora            rorb
            ror a           ror b
            ror     []

            tsta            tstb
            tst a           tst b
            tst     []

    Double Operand Instructions

            adca    []              adcb    []
            adc a   []              adc b   []

            adda    []      addb    []      addd    []
            add a   []      add b   []      add d   []

            anda    []              andb    []
            and a   []              and b   []

            bita    []              bitb    []
            bit a   []              bit b   []

            cmpa    []              cmpb    []
            cmp a   []              cmp b   []

            eora    []              eorb    []
            eor a   []              eor b   []

            ldaa    []              ldab    []
            lda a   []              lda b   []

            oraa    []              orab    []
            ora a   []              ora b   []

            sbca    []              sbcb    []
            sbc a   []              sbc b   []

            staa    []              stab    []
            sta a   []              sta b   []

            suba    []      subb    []      subd    []
            sub a   []      sub b   []      sub d   []

    Bit Manupulation Instructions

            bclr    [],#data
            bset    [],#data

            brclr   [],#data,label
            brset   [],#data,label

    Jump and Jump to Subroutine Instructions

            jmp     []              jsr     []

    Long Register Instructions

            cpx     []              cpy     []

            ldd     []              lds     []
            ldx     []              ldy     []

            std     []              sts     []
            stx     []              sty     []

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: April 2009