## Building ASxxxx and ASlink

### ... Building ASxxxx and ASlink

####

        ... Building ASxxxx and ASlink with Linux
        ... Building ASxxxx and ASlink with Cygwin
        ... Building ASxxxx and ASlink with DJGPP
        ... Building ASxxxx and ASlink with Symantec C/C++ 7.2
        ... Building ASxxxx and ASlink with Turbo C++ 3.0
        ... Building ASxxxx and ASlink with VC6
        ... Building ASxxxx and ASlink with VS2005
        ... Building ASxxxx and ASlink with VS2010
        ... Building ASxxxx and ASlink with Open Watcom
        ... Maintenance Files _prep.bat and _clean.bat
        ... Go to Documentation Index

####

       The assemblers and linker have been successfully compiled for
    Linux, DOS, and various flavors of Windows using the Linux  GCC,
    the Cygwin environment, the DJGPP environment, and the graphical
    user   interfaces   and    command    line    environments    of
    MS Visual C++ V6.0,   MS Visual Studio 2005,   Open Watcom V1.7,
    Symantec C/C++ V7.2, and Turbo C 3.0.

       Makefiles  for  Linux,  Cygwin,  DJGPP,  project  files and a
    makefile for Turbo C and psuedo makefiles and project files  for
    VC6, VS2005, Open Watcom and Symantec are available to build all
    the assemblers and the linker.

       Unpack  the  asxv5pxx.zip  file into an appropriate directory
    using the utility appropriate to your environment.  For  DOS  or
    Windows  the following command line will unpack the distribution
    zip file:

            pkunzip -d asxv5pxx.zip

    The  distribution  file  has  been  packed with DOS style end of
    lines (CR/LF), and UPPER CASE file names.  The Linux  make  file
    assumes  all  lower  case directories and file names.  For Linux
    the unpacking utility you choose should have an option to  force
    all  lower  case  directories / file names and convert the ascii
    files to local format.  On most systems  the  following  command
    should do the trick:

            unzip -L -a asxv5pxx.zip

    Some systems may require a -LL option to force all lower case.

       The  distribution  will  be  unpacked into the base directory
    'asxv5pxx' which will contain source directories for  each  sup-
    ported  processor  (as6800, asz80, ...), the machine independent
    source  (asxxsrc),  the  linker  source   (linksrc),   and   the
    miscellaneous sources (asxxmisc).  Other directories include the
    documentation (asxdoc), test file directory (asxtst),  html  do-
    cumentation  (asxhtml),  NoICE  support  files  (noice), various
    debug monitors that can be assembled with the ASxxxx  assemblers
    (asmasm),  project files for an application that uses the AS6809
    assembler and ASlink linker (project), and the packaging  direc-
    tory (zipper).

### ... Building ASxxxx and ASlink with Linux

####

       The  Linux  build  directory is /asxv5pxx/asxmak/linux/build.
    The makefile in this directory is compatible with the Linux  GNU
    make and GCC.  The command

            make clean

    will  remove  all  the  current  executable  files  in directory
    /asxv5pxx/asxmak/linux/exe and all the compiled  object  modules
    from the /asxv5pxx/asxmak/linux/build directory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

##### => Section Index

### ... Building ASxxxx and ASlink with Cygwin

####

       The  Cygwin build directory is \asxv5pxx\asxmak\cygwin\build.
    The makefile in this directory is compatible with the Cygwin GNU
    make and GCC.  The command

            make clean

    will  remove  all  the  current  executable  files  in directory
    \asxv5pxx\asxmak\cygwin\exe and all the compiled object  modules
    from the \asxv5pxx\asxmak\cygwin\build directory.  The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

##### => Section Index

### ... Building ASxxxx and ASlink with DJGPP

####

       The  DJGPP  build  directory is \asxv5pxx\asxmak\djgpp\build.
    The makefile in this directory is compatible with the DJGPP  GNU
    make and GCC.  The command

            make clean

    will  remove  all  the  current  executable  files  in directory
    \asxv5pxx\asxmak\djgpp\exe and all the compiled  object  modules
    from the \asxv5pxx\asxmak\djgpp\build directory.  The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

##### => Section Index

### ... Building ASxxxx and ASlink with Symantec C/C++ V7.2

####

       The  Symantec  product is no longer available but is included
    for historical reasons (the final version, 7.5,  was  introduced
    in  1996).   The  product had an excellent graphical user inter-
    face, built in editor, project manager, and supported  DOS,  Ex-
    tended  DOS  (the  executable  contained a built in DOS extender
    which was rendered unusable in Windows 2000, after service  pack
    2, or in Windows XP), Win95, and Windows NT.

    Graphical User Interface

       Each  ASxxxx Assembler has a series of project specific files
    (*.bro, *.def, *.dpd, *.lnk, *.mak, *.opn, and *.prj) located in
    in  the  subdirectory \asxv5pxx\asxmak\symantec\build.  You must
    enter the .prj filename into the Symantec IDE  and  then  select
    Project->Settings->Directories  and  change the include, target,
    and compiler output directories  to  match  your  configuration.
    After  these  changes have been made you will be able to compile
    the selected project.  These changes must  be  manually  entered
    for each project.

    Command Line Interface

       Before  the  command line interface can be used you must per-
    form the steps outlined in the 'Graphical  User  Interface'  in-
    structions above for each project you wish to build.

       Open      a      command     prompt     window     in     the
    \asxv5pxx\asxmak\symantec\build directory.   The  file  make.bat
    found  in  the directory can be used to invoke the Symantec com-
    mand line compiler.  The make.bat file assumes that the path  to
    the  compiler  directories has been set in the environment vari-
    able PATH.  Assuming the Symantec compiler has been installed in
    the  default location (C:\SC) the file _setpath.bat will set the
    PATH variable.  If this is not the case then the line

    PATH=C:\SC;C:\SC\BIN;C:\SC\INCLUDE;C:\SC\LIB

    must  be changed to match your environment.  The compiled object
    code      modules      will      be      placed      in      the
    \asxv5pxx\asxmak\symantec\build  directory  and  the  executable
    files will be placed in the \asxv5pxx\asxmak\symantec\exe direc-
    tory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

    The  Symantec  make utility , smake.exe, uses the information in
    the corresponding .mak files to compile and link the programs.

       The file _makeall.bat found in the directory can also be used
    to invoke the Symantec command line compiler.  The  _makeall.bat
    file calls the _setpath.bat file to set the path to the compiler
    directories in the environment variable PATH  and  then  invokes
    'make all'.

##### => Section Index

### ... Building ASxxxx and ASlink with Turbo C++ 3.0

####

       The  Borland  product  is  available in the Borland Turbo C++
    Suite which contains C++ Builder 1.0, Turbo C++ 4.5 for  Windows
    and  Turbo C++ 3.0 for DOS.  The DOS IDE will install and run on
    any version of Windows (including Windows Vista [Longhorn]).

    Graphical User Interface

       Each   ASxxxx   Assembler  has  two  project  specific  files
    (*.dsk and *.prj)     located      in      the      subdirectory
    \asxv5pxx\asxmak\turboc30\build.    You   must  enter  the  .prj
    filename into the Turbo C++ IDE:  enter Options->Directories and
    change  the  include and output directories to match your confi-
    guration.  After these changes have been made you will  be  able
    to compile the selected project.  These changes must be manually
    entered for each project.

    Command Line Interface

       Before  the  command line interface can be used you must per-
    form the steps outlined in the 'Graphical  User  Interface'  in-
    structions above for each project you wish to build.

       Open      a      command     prompt     window     in     the
    \asxv5pxx\asxmak\turboc30\build directory.  Assuming the Turbo C
    compiler  has been installed in the default location (C:\TC) the
    file _setpath.bat will set the PATH variable.  If  this  is  not
    the case then the line

    PATH=C:\TC;C:\TC\BIN;C:\TC\INCLUDE

    must  be changed to match your environment.  The compiled object
    code      modules      will      be      placed      in      the
    \asxv5pxx\asxmak\turboc30\build\  directory  and  the executable
    files will be placed in the \asxv5pxx\asxmak\turboc30\exe direc-
    tory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

    The Turbo C make utility uses the information in the correspond-
    ing .prj and .dsk files to compile and link the programs.

       The file _makeall.bat found in the directory can also be used
    to invoke the Turbo C command line compiler.   The  _makeall.bat
    file calls the _setpath.bat file to set the path to the compiler
    directories in the environment variable PATH  and  then  invokes
    'make all'.

##### => Section Index

### ... Building ASxxxx and ASlink with VC6

####

    Graphical User Interface

       Each  ASxxxx Assembler has a VC6 project file (*.dsw) located
    in a subdirectory of \asxv5pxx\asxmak\vc6\build.   Simply  enter
    this project filename into the VC6 IDE and build/rebuild the as-
    sembler.

    Command Line Interface

       Open      a      command     prompt     window     in     the
    \asxv5pxx\asxmak\vc6\build directory.  The file  make.bat  found
    in the directory can be used to invoke the VC6 command line com-
    piler.  The make.bat file assumes that the Visual  C++  compiler
    has  been installed in the default location.  If this is not the
    case then the line

    SET MS$DEV="C:\Program Files\Microsoft Visual Studio\
                   Common\MSDev98\Bin\msdev.exe"

    must  be changed to match your environment.  The compiled object
    code      modules      will      be      placed      in      the
    \asxv5pxx\asxmak\vc6\build\as----\release directory and the exe-
    cutable files will be  placed  in  the  \asxv5pxx\asxmak\vc6\exe
    directory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

    The  VC6  command line compiler uses the information in the cor-
    responding .dsw/.dsp files to compile and link the programs.

       The  command  'make clean' is not required or valid as a make
    of anything does a complete rebuild of the program.

##### => Section Index

### ... Building ASxxxx and ASlink with VS2005

####

    Graphical User Interface

       Each  ASxxxx  Assembler  has a VS2005 project file (*.vcproj)
    located in a subdirectory of \asxv5pxx\asxmak\vs05\build.   Sim-
    ply  enter  this  project  filename  into  the  VS2005  IDE  and
    build/rebuild the assembler.

    Command Line Interface

       Open      a      command     prompt     window     in     the
    \asxv5pxx\asxmak\vs05\build directory.  The file make.bat  found
    in  the  directory can be used to invoke the VS2005 command line
    compiler.  The make.bat file assumes that the  Visual  C++  com-
    piler  has  been  installed in the default location.  If this is
    not the case then the line

    SET VC$BUILD="C:\Program Files\Microsoft Visual Studio 8\
                     Common\MSDev98\Bin\msdev.exe"

    must  be changed to match your environment.  The compiled object
    code      modules      will      be      placed      in      the
    \asxv5pxx\asxmak\vs05\build\as----\release directory and the ex-
    ecutable files will be placed in  the  \asxv5pxx\asxmak\vs05\exe
    directory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

    The  VS2005  command  line  compiler uses the information in the
    corresponding .vcproj file to compile and link the programs.

       The  command  'make clean' is not required or valid as a make
    of anything does a complete rebuild of the program.

##### => Section Index

### ... Building ASxxxx and ASlink with VS2010

####

    Graphical User Interface

       Each  ASxxxx  Assembler has a VS2010 project file (*.vcxproj)
    located in a subdirectory of \asxv5pxx\asxmak\vs10\build.   Sim-
    ply  enter  this  project  filename  into  the  VS2010  IDE  and
    build/rebuild the assembler.

    Command Line Interface

       Open      a      command     prompt     window     in     the
    \asxv5pxx\asxmak\vs10\build directory.  The file make.bat  found
    in  the  directory can be used to invoke the VS2010 command line
    compiler.  The make.bat file assumes that the  Visual  C++  com-
    piler  has  been  installed in the default location.  If this is
    not the case then the line

    call "c:\Program Files (x86)\Microsoft Visual Studio 10.0\
                     VC\bin\vcvars32.bat"

    must  be changed to match your environment.  The compiled object
    code      modules      will      be      placed      in      the
    \asxv5pxx\asxmak\vs10\build\as----\release directory and the ex-
    ecutable files will be placed in  the  \asxv5pxx\asxmak\vs10\exe
    directory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

    The  VS2010  command  line  compiler uses the information in the
    corresponding .vcxproj file to compile and link the programs.

       The  command  'make clean' is not required or valid as a make
    of anything does a complete rebuild of the program.

##### => Section Index

### ... Building ASxxxx and ASlink with Open Watcom

####

    Graphical User Interface

       Each ASxxxx Assembler has a set of project files (.prj, .tgt,
    .mk,   .mk1,   and   .lk1)   located   in    the    subdirectory
    \asxv5pxx\asxmak\watcom\build.   You  will have to edit the pro-
    ject files to match your local file locations.

    Command Line Interface

       Open      a      command     prompt     window     in     the
    \asxv5pxx\asxmak\watcom\build directory.   Assuming  the  Watcom
    compiler  has been installed in the default location (C:\WATCOM)
    the file _setpath.bat will set the PATH variable.   If  this  is
    not the case then the line

    PATH=C:\WATCOM\BINNT;C:\WATCOM\BINW

    must  be changed to match your environment.  The compiled object
    code      modules      will      be      placed      in      the
    \asxv5pxx\asxmak\watcom\build\   directory  and  the  executable
    files will be placed in the  \asxv5pxx\asxmak\watcom\exe  direc-
    tory.

       The command

            make all

    will compile and link all the ASxxxx assemblers, the ASlink pro-
    gram, and the utility programs asxscn and asxcnv.  The make file
    can make a single program by invoking make with the specific as-
    sembler, linker, or utility you wish to build:

            make aslink

    The  Watcom command line compiler wmake.exe uses the information
    in the corresponding project files to compile and link the  pro-
    grams.

       The file _makeall.bat found in the directory can also be used
    to invoke the Watcom command line  compiler.   The  _makeall.bat
    file calls the _setpath.bat file to set the path to the compiler
    directories in the environment variable PATH  and  then  invokes
    'make all'.

       The  command  'make clean' is not required or valid as a make
    of anything does a complete rebuild of the program.

##### => Section Index

### ... Maintenace Files _prep.bat and _clean.bat

####

       Each  of  the  build  directories have two maintenance files:
    _prep.bat and _clean.bat.  The command file  _prep.bat  prepares
    the particular compiler directories for distribution by removing
    all exteraneous files but keeping  the  final  compiled  execut-
    ables.   The  _clean.bat command file performs the same function
    as _prep.bat and removes the compiled executables.

##### => Section Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: August 2012